--------------------------------------------------------------------------------
FtMscLib.dll Version  01.04.24  (2009/09/21)
FtLogLevel= 0
10:43:19:812, Initialization of Library 'ftMscLib.dll' ...

INFO:   size FTX1_SHMIFINFO   = 64
INFO:   size FTX1_STATE       = 36
INFO:   size FTX1_CONFIG      = 88
INFO:   size FTX1_INPUT       = 44
INFO:   size FTX1_OUTPUT      = 36
INFO:   size FTX1_DISPLAY     = 76
INFO:   size TRANSFER_STATUS  = 4
INFO:   size CHANGE_STATE     = 8
INFO:   size RP_TIMER         = 12
INFO:   size MOTOR            = 24
INFO:   size INPUT_SIM        = 4
INFO:   size HOOK_TABLE       = 16
INFO:   RESERVE_SIZE          = 100
INFO:   size FISH_X1_TRANSFER = 512
INFO: size IF08_MAX           = 9
INFO: size IF08_TRANSFER      = 4608

10:43:19:812, Creating event objects...
10:43:19:812, Starting thread [WaitMmRpTmEvent]...
10:43:19:812,   [WaitMmRpTmEvent] started, hRpTmThrWait= 432
10:43:19:812, Starting thread [WaitMmEvent]...
10:43:19:812,   [WaitMmEventThread] started, hThrWait= 436
10:43:19:812, Starting thread [FtRequestThread]...
10:43:19:812,   [FtRequestThread] started, hThrRequest= 440
10:43:19:812, Starting MMTimer... (mmRpTimerId= 16)
10:43:19:812, ftMscLib is initialized ...

10:43:22:609, OpenComDevice(), comStr= COM3
10:43:22:609, CSerial::Open, open 'COM3' resource ...
10:43:22:609, CSerial::Open, COM 'COM3' (baudr= 38400)  opened...
10:43:22:640, ftxOpenComDevice(), ftHandle= 592
10:43:22:640, Starting thread [ReadComThread]...
10:43:22:640, Thread [ReadComThread] started..., hComRead= 596, IdComReadThread= 2888
10:43:22:640, Open Fish.X1 connection...
10:43:22:656, [SetFishX1InfoData] shmId= 0
10:43:22:656,   Hostname          : ROBO TX-405
10:43:22:656,   BtAddress         : 00:13:7B:54:08:AB
10:43:22:656,   Hardware Release  : C
10:43:22:656,   Firmware Version  : V 1.18
10:43:22:656,   SharedMemoryStart : 0x20000204
10:43:22:656,   AppAreaStart      : 0x30700000
10:43:22:656,   AppAreaSize       : 0x000D0000
10:43:22:656, Initialization output and config area...
10:43:22:656, Info Master/Slave alive:  M  0  0  0  0  0  0  0  0
10:43:22:656, InitTransferValues, Initialization of TransferArea (output)...
10:43:22:750, SendRemoteCmd, XM_START: send remote command: 'get_ser_num'
10:43:22:750, SendRemoteCmd, XM_GET_PROMPT: ROBO TX prompt received...
10:43:22:750, serial_number= [0001983800]
10:45:04:937, RoboTxFwUpdate, fwpath= [C:\ROBO PRO 2142- sofware 2011\ROBOPro\ROBO Interface Firmware\TXController_01_18]
10:45:04:937, ReadFirmwareFiles, nFwFiles= 5
10:45:04:937, 0: boot_fs.img
10:45:04:937, 1: Deutsch.lang
10:45:04:937, 2: ft_robo_if08.eno
10:45:04:937, 3: Hrvatski.lang
10:45:04:937, 4: RoboLib.dll
10:45:04:937, Starting Thread FwUpdThread...
10:45:05:046, FirmwareVersion: [1.18]
10:45:05:046, FirmwareVersion: MainFwVer= 1, SubFwVer= 18
10:45:05:046, GetFwUpdSteps, Firmware Update Steps= 19
10:45:05:046, Status: FTLIB_FWUPD_STARTING, Firmware Update starts...
10:45:05:046, File phase0.bin not found in list...
INFO: FtFileUpload, fname= C:\ROBO PRO 2142- sofware 2011\ROBOPro\ROBO Interface Firmware\TXController_01_18\boot_fs.img
INFO: FtFileUpload, Device= 0, FileName= boot_fs.img, size= 74404
10:45:05:156, Starting Thread IfUploadFile...
10:45:05:156, IfUploadFile, XM_START: send upload command
10:45:05:156, Starting Upload ...xrecv /ramdisk/"boot_fs.img" 74404
10:45:05:156, cbFileUpload, status == FTLIB_ERR_UPLOAD_START
10:45:05:656, IfUploadFile, XM_WAIT_UPLOAD: received 'C'...
10:45:06:156, File Upload successful...
10:45:06:156, cbFileUpload, status == FTLIB_ERR_UPLOAD_DONE
10:45:06:156, Closing thread IfUploadFile...
10:45:06:156, Remote: clean_disk flash
10:45:06:250, SendRemoteCmd, XM_START: send remote command: 'clean_disk flash'
10:45:06:265, SendRemoteCmd, XM_GET_PROMPT: ROBO TX prompt received...
10:45:06:265, Remote: auto_sync off
10:45:06:359, SendRemoteCmd, XM_START: send remote command: 'auto_sync off'
10:45:06:359, SendRemoteCmd, XM_GET_PROMPT: ROBO TX prompt received...
INFO: FtFileUpload, fname= C:\ROBO PRO 2142- sofware 2011\ROBOPro\ROBO Interface Firmware\TXController_01_18\ft_robo_if08.eno
INFO: FtFileUpload, Device= 1, FileName= ft_robo_if08.eno, size= 617300
10:45:06:468, Starting Thread IfUploadFile...
10:45:06:468, IfUploadFile, XM_START: send upload command
10:45:06:468, Starting Upload ...xrecv /flash/"ft_robo_if08.eno" 617300
10:45:06:468, cbFileUpload, status == FTLIB_ERR_UPLOAD_START
10:45:06:968, IfUploadFile, XM_WAIT_UPLOAD: received 'C'...
10:45:10:796, File Upload successful...
10:45:10:796, cbFileUpload, status == FTLIB_ERR_UPLOAD_DONE
10:45:10:796, Closing thread IfUploadFile...
INFO: FtFileUpload, fname= C:\ROBO PRO 2142- sofware 2011\ROBOPro\ROBO Interface Firmware\TXController_01_18\RoboLib.dll
INFO: FtFileUpload, Device= 1, FileName= RoboLib.dll, size= 74528
10:45:10:906, Starting Thread IfUploadFile...
10:45:10:906, IfUploadFile, XM_START: send upload command
10:45:10:906, Starting Upload ...xrecv /flash/"RoboLib.dll" 74528
10:45:10:906, cbFileUpload, status == FTLIB_ERR_UPLOAD_START
10:45:11:406, IfUploadFile, XM_WAIT_UPLOAD: received 'C'...
10:45:11:921, File Upload successful...
10:45:11:921, cbFileUpload, status == FTLIB_ERR_UPLOAD_DONE
10:45:11:921, Closing thread IfUploadFile...
INFO: FtFileUpload, fname= C:\ROBO PRO 2142- sofware 2011\ROBOPro\ROBO Interface Firmware\TXController_01_18\Deutsch.lang
INFO: FtFileUpload, Device= 1, FileName= Deutsch.lang, size= 1990
10:45:12:015, Starting Thread IfUploadFile...
10:45:12:015, IfUploadFile, XM_START: send upload command
10:45:12:015, Starting Upload ...xrecv /flash/"Deutsch.lang" 1990
10:45:12:015, cbFileUpload, status == FTLIB_ERR_UPLOAD_START
10:45:12:515, IfUploadFile, XM_WAIT_UPLOAD: received 'C'...
10:45:12:593, File Upload successful...
10:45:12:593, cbFileUpload, status == FTLIB_ERR_UPLOAD_DONE
10:45:12:593, Closing thread IfUploadFile...
INFO: FtFileUpload, fname= C:\ROBO PRO 2142- sofware 2011\ROBOPro\ROBO Interface Firmware\TXController_01_18\Hrvatski.lang
INFO: FtFileUpload, Device= 1, FileName= Hrvatski.lang, size= 1999
10:45:12:687, Starting Thread IfUploadFile...
10:45:12:687, IfUploadFile, XM_START: send upload command
10:45:12:687, Starting Upload ...xrecv /flash/"Hrvatski.lang" 1999
10:45:12:687, cbFileUpload, status == FTLIB_ERR_UPLOAD_START
10:45:13:187, IfUploadFile, XM_WAIT_UPLOAD: received 'C'...
10:45:13:234, File Upload successful...
10:45:13:234, cbFileUpload, status == FTLIB_ERR_UPLOAD_DONE
10:45:13:234, Closing thread IfUploadFile...
10:45:13:234, File .lang not found in list...
10:45:13:234, Remote: flush_disk flash
10:45:13:328, SendRemoteCmd, XM_START: send remote command: 'flush_disk flash'
10:45:17:187, SendRemoteCmd, XM_GET_PROMPT: ROBO TX prompt received...
10:45:17:187, Copy Firmware Files:  copy /flash/ft_robo_if08.eno /system/ft_robo_if08.eno
10:45:17:187, Remote: copy /flash/ft_robo_if08.eno /system/ft_robo_if08.eno
10:45:17:281, SendRemoteCmd, XM_START: send remote command: 'copy /flash/ft_robo_if08.eno /system/ft_robo_if08.eno'
10:45:17:781, SendRemoteCmd, XM_GET_PROMPT: ROBO TX prompt received...
10:45:17:781, Copy Firmware Files:  copy /flash/RoboLib.dll /system/RoboLib.dll
10:45:17:781, Remote: copy /flash/RoboLib.dll /system/RoboLib.dll
10:45:17:875, SendRemoteCmd, XM_START: send remote command: 'copy /flash/RoboLib.dll /system/RoboLib.dll'
10:45:17:968, SendRemoteCmd, XM_GET_PROMPT: ROBO TX prompt received...
10:45:17:968, Copy Firmware Files:  copy /flash/Deutsch.lang /system/Deutsch.lang
10:45:17:968, Remote: copy /flash/Deutsch.lang /system/Deutsch.lang
10:45:18:078, SendRemoteCmd, XM_START: send remote command: 'copy /flash/Deutsch.lang /system/Deutsch.lang'
10:45:18:109, SendRemoteCmd, XM_GET_PROMPT: ROBO TX prompt received...
10:45:18:109, Copy Firmware Files:  copy /flash/Hrvatski.lang /system/Hrvatski.lang
10:45:18:109, Remote: copy /flash/Hrvatski.lang /system/Hrvatski.lang
10:45:18:203, SendRemoteCmd, XM_START: send remote command: 'copy /flash/Hrvatski.lang /system/Hrvatski.lang'
10:45:18:234, SendRemoteCmd, XM_GET_PROMPT: ROBO TX prompt received...
10:45:18:234, File .lang not found in list...
10:45:18:234, Remote: flush_disk system
10:45:18:328, SendRemoteCmd, XM_START: send remote command: 'flush_disk system'
10:45:21:796, SendRemoteCmd, XM_GET_PROMPT: ROBO TX prompt received...
10:45:21:796, Delete Firmware Files:  del /flash/ft_robo_if08.eno
10:45:21:796, Remote: del /flash/ft_robo_if08.eno
10:45:21:890, SendRemoteCmd, XM_START: send remote command: 'del /flash/ft_robo_if08.eno'
10:45:21:906, SendRemoteCmd, XM_GET_PROMPT: ROBO TX prompt received...
10:45:21:906, Delete Firmware Files:  del /flash/RoboLib.dll
10:45:21:906, Remote: del /flash/RoboLib.dll
10:45:22:000, SendRemoteCmd, XM_START: send remote command: 'del /flash/RoboLib.dll'
10:45:22:000, SendRemoteCmd, XM_GET_PROMPT: ROBO TX prompt received...
10:45:22:000, Delete Firmware Files:  del /flash/Deutsch.lang
10:45:22:000, Remote: del /flash/Deutsch.lang
10:45:22:109, SendRemoteCmd, XM_START: send remote command: 'del /flash/Deutsch.lang'
10:45:22:109, SendRemoteCmd, XM_GET_PROMPT: ROBO TX prompt received...
10:45:22:109, Delete Firmware Files:  del /flash/Hrvatski.lang
10:45:22:109, Remote: del /flash/Hrvatski.lang
10:45:22:218, SendRemoteCmd, XM_START: send remote command: 'del /flash/Hrvatski.lang'
10:45:22:218, SendRemoteCmd, XM_GET_PROMPT: ROBO TX prompt received...
10:45:22:218, File .lang not found in list...
10:45:22:218, Remote: flush_disk flash
10:45:22:328, SendRemoteCmd, XM_START: send remote command: 'flush_disk flash'
10:45:25:968, SendRemoteCmd, XM_GET_PROMPT: ROBO TX prompt received...
10:45:25:968, Remote: auto_sync on
10:45:26:078, SendRemoteCmd, XM_START: send remote command: 'auto_sync on'
10:45:26:078, SendRemoteCmd, XM_GET_PROMPT: ROBO TX prompt received...
10:45:26:078, Status: FTLIB_FWUPD_FINISHED, Firmware Update finished...
10:45:26:078, Closing thread FwUpdThread..., exitCode= 0
10:51:09:953, CloseComDevice, ftHandle= 592
10:51:09:953, cancel thread [ReadComThread]...
10:51:10:000, Stopped MmTimer (mmRpTimerId= 16)...
10:51:10:000, Threads terminated...
10:51:10:000, Closing event handles...
10:51:10:000, ftMscLib closed.
