--------------------------------------------------------------------------------
FtMscLib.dll Version  01.04.24  (2009/09/21)
FtLogLevel= 0
11:00:59:453, Initialization of Library 'ftMscLib.dll' ...

INFO:   size FTX1_SHMIFINFO   = 64
INFO:   size FTX1_STATE       = 36
INFO:   size FTX1_CONFIG      = 88
INFO:   size FTX1_INPUT       = 44
INFO:   size FTX1_OUTPUT      = 36
INFO:   size FTX1_DISPLAY     = 76
INFO:   size TRANSFER_STATUS  = 4
INFO:   size CHANGE_STATE     = 8
INFO:   size RP_TIMER         = 12
INFO:   size MOTOR            = 24
INFO:   size INPUT_SIM        = 4
INFO:   size HOOK_TABLE       = 16
INFO:   RESERVE_SIZE          = 100
INFO:   size FISH_X1_TRANSFER = 512
INFO: size IF08_MAX           = 9
INFO: size IF08_TRANSFER      = 4608

11:00:59:453, Creating event objects...
11:00:59:453, Starting thread [WaitMmRpTmEvent]...
11:00:59:453,   [WaitMmRpTmEvent] started, hRpTmThrWait= 432
11:00:59:453, Starting thread [WaitMmEvent]...
11:00:59:453,   [WaitMmEventThread] started, hThrWait= 436
11:00:59:453, Starting thread [FtRequestThread]...
11:00:59:453,   [FtRequestThread] started, hThrRequest= 440
11:00:59:453, Starting MMTimer... (mmRpTimerId= 16)
11:00:59:453, ftMscLib is initialized ...

11:01:01:859, OpenComDevice(), comStr= COM3
11:01:01:859, CSerial::Open, open 'COM3' resource ...
11:01:01:859, CSerial::Open, COM 'COM3' (baudr= 38400)  opened...
11:01:01:906, ftxOpenComDevice(), ftHandle= 592
11:01:01:906, Starting thread [ReadComThread]...
11:01:01:906, Thread [ReadComThread] started..., hComRead= 596, IdComReadThread= 2152
11:01:01:906, Open Fish.X1 connection...
11:01:01:906, [SetFishX1InfoData] shmId= 0
11:01:01:906,   Hostname          : ROBO TX-405
11:01:01:906,   BtAddress         : 00:13:7B:54:08:AB
11:01:01:906,   Hardware Release  : C
11:01:01:906,   Firmware Version  : V 1.18
11:01:01:906,   SharedMemoryStart : 0x20000204
11:01:01:906,   AppAreaStart      : 0x30700000
11:01:01:906,   AppAreaSize       : 0x000D0000
11:01:01:906, Initialization output and config area...
11:01:01:906, Info Master/Slave alive:  M  0  0  0  0  0  0  0  0
11:01:01:906, InitTransferValues, Initialization of TransferArea (output)...
11:01:02:015, SendRemoteCmd, XM_START: send remote command: 'get_ser_num'
11:01:02:015, SendRemoteCmd, XM_GET_PROMPT: ROBO TX prompt received...
11:01:02:015, serial_number= [0001983800]
11:01:15:781, RoboTxFwUpdate, fwpath= [C:\ROBO PRO 2142- sofware 2011\ROBOPro\ROBO Interface Firmware\TXController_01_18]
11:01:15:781, ReadFirmwareFiles, nFwFiles= 5
11:01:15:781, 0: boot_fs.img
11:01:15:781, 1: Deutsch.lang
11:01:15:781, 2: ft_robo_if08.eno
11:01:15:781, 3: Hrvatski.lang
11:01:15:781, 4: RoboLib.dll
11:01:15:781, Starting Thread FwUpdThread...
11:01:15:875, FirmwareVersion: [1.18]
11:01:15:875, FirmwareVersion: MainFwVer= 1, SubFwVer= 18
11:01:15:875, GetFwUpdSteps, Firmware Update Steps= 19
11:01:15:875, Status: FTLIB_FWUPD_STARTING, Firmware Update starts...
11:01:15:875, File phase0.bin not found in list...
INFO: FtFileUpload, fname= C:\ROBO PRO 2142- sofware 2011\ROBOPro\ROBO Interface Firmware\TXController_01_18\boot_fs.img
INFO: FtFileUpload, Device= 0, FileName= boot_fs.img, size= 74404
11:01:15:984, Starting Thread IfUploadFile...
11:01:15:984, IfUploadFile, XM_START: send upload command
11:01:15:984, Starting Upload ...xrecv /ramdisk/"boot_fs.img" 74404
11:01:15:984, cbFileUpload, status == FTLIB_ERR_UPLOAD_START
11:01:16:484, IfUploadFile, XM_WAIT_UPLOAD: received 'C'...
11:01:16:968, File Upload successful...
11:01:16:968, cbFileUpload, status == FTLIB_ERR_UPLOAD_DONE
11:01:16:968, Closing thread IfUploadFile...
11:01:16:968, Remote: clean_disk flash
11:01:17:062, SendRemoteCmd, XM_START: send remote command: 'clean_disk flash'
11:01:17:062, SendRemoteCmd, XM_GET_PROMPT: ROBO TX prompt received...
11:01:17:062, Remote: auto_sync off
11:01:17:171, SendRemoteCmd, XM_START: send remote command: 'auto_sync off'
11:01:17:171, SendRemoteCmd, XM_GET_PROMPT: ROBO TX prompt received...
INFO: FtFileUpload, fname= C:\ROBO PRO 2142- sofware 2011\ROBOPro\ROBO Interface Firmware\TXController_01_18\ft_robo_if08.eno
INFO: FtFileUpload, Device= 1, FileName= ft_robo_if08.eno, size= 617300
11:01:17:265, Starting Thread IfUploadFile...
11:01:17:265, IfUploadFile, XM_START: send upload command
11:01:17:265, Starting Upload ...xrecv /flash/"ft_robo_if08.eno" 617300
11:01:17:265, cbFileUpload, status == FTLIB_ERR_UPLOAD_START
11:01:17:781, IfUploadFile, XM_WAIT_UPLOAD: received 'C'...
11:01:21:593, File Upload successful...
11:01:21:593, cbFileUpload, status == FTLIB_ERR_UPLOAD_DONE
11:01:21:593, Closing thread IfUploadFile...
INFO: FtFileUpload, fname= C:\ROBO PRO 2142- sofware 2011\ROBOPro\ROBO Interface Firmware\TXController_01_18\RoboLib.dll
INFO: FtFileUpload, Device= 1, FileName= RoboLib.dll, size= 74528
11:01:21:687, Starting Thread IfUploadFile...
11:01:21:687, IfUploadFile, XM_START: send upload command
11:01:21:687, Starting Upload ...xrecv /flash/"RoboLib.dll" 74528
11:01:21:687, cbFileUpload, status == FTLIB_ERR_UPLOAD_START
11:01:22:203, IfUploadFile, XM_WAIT_UPLOAD: received 'C'...
11:01:22:687, File Upload successful...
11:01:22:687, cbFileUpload, status == FTLIB_ERR_UPLOAD_DONE
11:01:22:687, Closing thread IfUploadFile...
INFO: FtFileUpload, fname= C:\ROBO PRO 2142- sofware 2011\ROBOPro\ROBO Interface Firmware\TXController_01_18\Deutsch.lang
INFO: FtFileUpload, Device= 1, FileName= Deutsch.lang, size= 1990
11:01:22:796, Starting Thread IfUploadFile...
11:01:22:796, IfUploadFile, XM_START: send upload command
11:01:22:796, Starting Upload ...xrecv /flash/"Deutsch.lang" 1990
11:01:22:796, cbFileUpload, status == FTLIB_ERR_UPLOAD_START
11:01:23:296, IfUploadFile, XM_WAIT_UPLOAD: received 'C'...
11:01:23:343, File Upload successful...
11:01:23:343, cbFileUpload, status == FTLIB_ERR_UPLOAD_DONE
11:01:23:343, Closing thread IfUploadFile...
INFO: FtFileUpload, fname= C:\ROBO PRO 2142- sofware 2011\ROBOPro\ROBO Interface Firmware\TXController_01_18\Hrvatski.lang
INFO: FtFileUpload, Device= 1, FileName= Hrvatski.lang, size= 2007
11:01:23:437, Starting Thread IfUploadFile...
11:01:23:437, IfUploadFile, XM_START: send upload command
11:01:23:437, Starting Upload ...xrecv /flash/"Hrvatski.lang" 2007
11:01:23:437, cbFileUpload, status == FTLIB_ERR_UPLOAD_START
11:01:23:937, IfUploadFile, XM_WAIT_UPLOAD: received 'C'...
11:01:23:984, File Upload successful...
11:01:23:984, cbFileUpload, status == FTLIB_ERR_UPLOAD_DONE
11:01:23:984, Closing thread IfUploadFile...
11:01:23:984, File .lang not found in list...
11:01:23:984, Remote: flush_disk flash
11:01:24:078, SendRemoteCmd, XM_START: send remote command: 'flush_disk flash'
11:01:27:734, SendRemoteCmd, XM_GET_PROMPT: ROBO TX prompt received...
11:01:27:734, Copy Firmware Files:  copy /flash/ft_robo_if08.eno /system/ft_robo_if08.eno
11:01:27:734, Remote: copy /flash/ft_robo_if08.eno /system/ft_robo_if08.eno
11:01:27:843, SendRemoteCmd, XM_START: send remote command: 'copy /flash/ft_robo_if08.eno /system/ft_robo_if08.eno'
11:01:28:328, SendRemoteCmd, XM_GET_PROMPT: ROBO TX prompt received...
11:01:28:328, Copy Firmware Files:  copy /flash/RoboLib.dll /system/RoboLib.dll
11:01:28:328, Remote: copy /flash/RoboLib.dll /system/RoboLib.dll
11:01:28:437, SendRemoteCmd, XM_START: send remote command: 'copy /flash/RoboLib.dll /system/RoboLib.dll'
11:01:28:531, SendRemoteCmd, XM_GET_PROMPT: ROBO TX prompt received...
11:01:28:531, Copy Firmware Files:  copy /flash/Deutsch.lang /system/Deutsch.lang
11:01:28:531, Remote: copy /flash/Deutsch.lang /system/Deutsch.lang
11:01:28:625, SendRemoteCmd, XM_START: send remote command: 'copy /flash/Deutsch.lang /system/Deutsch.lang'
11:01:28:656, SendRemoteCmd, XM_GET_PROMPT: ROBO TX prompt received...
11:01:28:656, Copy Firmware Files:  copy /flash/Hrvatski.lang /system/Hrvatski.lang
11:01:28:656, Remote: copy /flash/Hrvatski.lang /system/Hrvatski.lang
11:01:28:750, SendRemoteCmd, XM_START: send remote command: 'copy /flash/Hrvatski.lang /system/Hrvatski.lang'
11:01:28:781, SendRemoteCmd, XM_GET_PROMPT: ROBO TX prompt received...
11:01:28:781, File .lang not found in list...
11:01:28:781, Remote: flush_disk system
11:01:28:890, SendRemoteCmd, XM_START: send remote command: 'flush_disk system'
11:01:32:546, SendRemoteCmd, XM_GET_PROMPT: ROBO TX prompt received...
11:01:32:546, Delete Firmware Files:  del /flash/ft_robo_if08.eno
11:01:32:546, Remote: del /flash/ft_robo_if08.eno
11:01:32:640, SendRemoteCmd, XM_START: send remote command: 'del /flash/ft_robo_if08.eno'
11:01:32:656, SendRemoteCmd, XM_GET_PROMPT: ROBO TX prompt received...
11:01:32:656, Delete Firmware Files:  del /flash/RoboLib.dll
11:01:32:656, Remote: del /flash/RoboLib.dll
11:01:32:750, SendRemoteCmd, XM_START: send remote command: 'del /flash/RoboLib.dll'
11:01:32:765, SendRemoteCmd, XM_GET_PROMPT: ROBO TX prompt received...
11:01:32:765, Delete Firmware Files:  del /flash/Deutsch.lang
11:01:32:765, Remote: del /flash/Deutsch.lang
11:01:32:859, SendRemoteCmd, XM_START: send remote command: 'del /flash/Deutsch.lang'
11:01:32:875, SendRemoteCmd, XM_GET_PROMPT: ROBO TX prompt received...
11:01:32:875, Delete Firmware Files:  del /flash/Hrvatski.lang
11:01:32:875, Remote: del /flash/Hrvatski.lang
11:01:32:968, SendRemoteCmd, XM_START: send remote command: 'del /flash/Hrvatski.lang'
11:01:32:984, SendRemoteCmd, XM_GET_PROMPT: ROBO TX prompt received...
11:01:32:984, File .lang not found in list...
11:01:32:984, Remote: flush_disk flash
11:01:33:078, SendRemoteCmd, XM_START: send remote command: 'flush_disk flash'
11:01:36:718, SendRemoteCmd, XM_GET_PROMPT: ROBO TX prompt received...
11:01:36:718, Remote: auto_sync on
11:01:36:828, SendRemoteCmd, XM_START: send remote command: 'auto_sync on'
11:01:36:828, SendRemoteCmd, XM_GET_PROMPT: ROBO TX prompt received...
11:01:36:828, Status: FTLIB_FWUPD_FINISHED, Firmware Update finished...
11:01:36:828, Closing thread FwUpdThread..., exitCode= 0
11:01:39:968, CloseComDevice, ftHandle= 592
11:01:39:968, cancel thread [ReadComThread]...
11:01:40:015, Stopped MmTimer (mmRpTimerId= 16)...
11:01:40:015, Threads terminated...
11:01:40:015, Closing event handles...
11:01:40:015, ftMscLib closed.
